**Irrigation warranty**

All materials are guaranteed to be commercial grade as specified, and work shall be performed in a timely manner according to industry standards.  All materials carry manufacturer's warranties of at least one year.

Choate USA provides a one-year guarantee on all labor.  Acts of man (such as vehicle damage or third party manipulations) and nature (such as lightning) are not defined as warranty situations.

Choate USA is not responsible for freeze damage to mandated above ground backflow prevention devises.

Full coverage of planned irrigated areas is unconditionally guaranteed.

Automatic control panel will be Rainbird or Hunter.

All heads and valves to be Rainbird or Hunter with flexible swing joints.

Master valve to be installed after backflow prevention device.

Thank you!

**Nita Hunter**
Builder / Residential Sales Manager
**Choate USA**214-687-1097[www.ChoateUSA.com](http://www.ChoateUSA.com)